JAPANESE INDUSTRIAL STANDARD

JIS G 3323：2019

Hot-dip zinc-aluminium-magnesium alloy-coated steel sheet and strip

May, 2021

ERRATUM

|  |  |  |  |
| --- | --- | --- | --- |
| Page | Position | Error | Correct |
| 25 | Clause 17 | The report shall include the type of equivalent coating thickness  applied, which is given in Table 14. | The report shall include the type of equivalent coating thickness  applied, which is given in Table 15. |